{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Faq"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Faq","index":0,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["N.ro","Domanda","Risposta"]
[1,"Con riferimento alla procedura in oggetto si inviano le seguenti richieste di chiarimento.\r\n \r\nL'art.6 del Capitolato Speciale richiede come caratteristiche minime:\r\n1) diametro tamburo vagliante: 2100 mm.\r\n2) Peso totale ammissibile della macchina: 16.000 kg.\r\n \r\nSi chiede conferma del fatto che la misura del diametro del tamburo vagliante sia riferita a quella esterna.\r\n \r\nSi chiede conferma che il peso di 16.000 kg sia quello minimo ammissibile, essendo possibile offrire macchine più robuste e pesanti di 16.000 kg.\r\n","A riscontro della vostra richiesta di chiarimento si conferma che la misura del diametro del tamburo vagliante è riferita a quella esterna.\r\nSi conferma, inoltre, che il peso di 16.000 kg è quello minimo ammissibile.\r\n\r\nCordiali saluti\r\n\r\nIl R.U.P.\r\n(ing. Piero Bertolusso)"]